{"text_format":"3","workbook":"xls","n_sheets":3,"sheets":["Sheet1","Sheet2","Sheet3"],"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Sheet1","index":0,"n_rows":232,"n_cols":7,"rows_kept":232,"merged":[[0,0,0,6],[1,0,1,3],[1,4,1,6],[2,0,4,0],[2,1,4,1],[2,2,4,2],[2,3,4,4],[2,5,4,5],[2,6,4,6],[5,3,5,4],[6,3,6,4],[7,3,7,4],[8,3,8,4],[9,3,9,4],[10,3,10,4],[11,3,11,4],[12,3,12,4],[13,3,13,4],[14,3,14,4],[15,3,15,4],[16,3,16,4],[17,3,17,4],[18,0,18,6],[19,0,19,6],[20,0,20,3],[20,4,20,6],[21,0,21,6],[22,0,22,3],[22,4,22,6],[23,0,25,0],[23,1,25,1],[23,2,25,2],[23,3,25,4],[23,5,25,5],[23,6,25,6],[26,3,26,4],[27,3,27,4],[28,3,28,4],[29,3,29,4],[30,3,30,4],[31,3,31,4],[32,3,32,4],[33,3,33,4],[34,3,34,4],[35,3,35,4],[36,3,36,4],[37,0,37,6],[38,0,38,6],[39,0,39,3],[39,4,39,6],[40,0,40,6],[41,0,41,3],[41,4,41,6],[42,0,44,0],[42,1,44,1],[42,2,44,2],[42,3,44,4],[42,5,44,5],[42,6,44,6],[45,3,45,4],[46,3,46,4],[47,3,47,4],[48,3,48,4],[49,3,49,4],[50,3,50,4],[51,3,51,4],[52,3,52,4],[53,3,53,4],[54,3,54,4],[55,0,55,6],[56,0,56,6],[57,0,57,3],[57,4,57,6],[58,0,58,6],[59,0,59,3],[59,4,59,6],[60,0,62,0],[60,1,62,1],[60,2,62,2],[60,3,62,4],[60,5,62,5],[60,6,62,6],[63,3,63,4],[64,3,64,4],[65,3,65,4],[66,3,66,4],[67,3,67,4],[68,3,68,4],[69,3,69,4],[70,3,70,4],[71,3,71,4],[72,3,72,4],[73,3,73,4],[74,3,74,4],[75,3,75,4],[76,3,76,4],[77,3,77,4],[78,3,78,4],[79,3,79,4],[80,3,80,4],[81,3,81,4],[82,0,82,6],[83,0,83,6],[84,0,84,3],[84,4,84,6],[85,0,85,6],[86,0,86,3],[86,4,86,6],[87,0,89,0],[87,1,89,1],[87,2,89,2],[87,3,89,4],[87,5,89,5],[87,6,89,6],[90,3,90,4],[91,3,91,4],[92,3,92,4],[93,3,93,4],[94,3,94,4],[95,3,95,4],[96,3,96,4],[97,3,97,4],[98,3,98,4],[99,3,99,4],[100,3,100,4],[101,3,101,4],[102,3,102,4],[103,3,103,4],[104,3,104,4],[105,3,105,4],[106,3,106,4],[107,3,107,4],[108,0,108,6],[109,0,109,3],[109,4,109,6],[110,0,112,0],[110,1,112,1],[110,2,112,2],[110,3,112,4],[110,5,112,5],[110,6,112,6],[113,3,113,4],[114,3,114,4],[115,3,115,4],[116,3,116,4],[117,3,117,4],[118,3,118,4],[119,3,119,4],[120,3,120,4],[121,3,121,4],[122,3,122,4],[123,3,123,4],[124,0,124,6],[125,0,125,6],[126,0,126,3],[126,4,126,6],[127,0,127,6],[128,0,128,3],[128,4,128,6],[129,0,131,0],[129,1,131,1],[129,2,131,2],[129,3,131,4],[129,5,131,5],[129,6,131,6],[132,3,132,4],[133,3,133,4],[134,3,134,4],[135,3,135,4],[136,3,136,4],[137,3,137,4],[138,3,138,4],[139,3,139,4],[140,3,140,4],[141,3,141,4],[142,3,142,4],[143,3,143,4],[144,3,144,4],[145,3,145,4],[146,0,146,6],[147,0,147,6],[148,0,148,3],[148,4,148,6],[149,0,149,6],[150,0,150,3],[150,4,150,6],[151,0,153,0],[151,1,153,1],[151,2,153,2],[151,3,153,4],[151,5,153,5],[151,6,153,6],[154,3,154,4],[155,3,155,4],[156,3,156,4],[157,3,157,4],[158,3,158,4],[159,3,159,4],[160,3,160,4],[161,3,161,4],[162,3,162,4],[163,3,163,4],[164,3,164,4],[165,3,165,4],[166,3,166,4],[167,3,167,4],[168,3,168,4],[169,0,169,6],[170,0,170,6],[171,0,171,3],[171,4,171,6],[172,0,172,6],[173,0,173,3],[173,4,173,6],[174,0,176,0],[174,1,176,1],[174,2,176,2],[174,3,176,4],[174,5,176,5],[174,6,176,6],[177,3,177,4],[178,3,178,4],[179,3,179,4],[180,3,180,4],[181,3,181,4],[182,3,182,4],[183,3,183,4],[184,3,184,4],[185,3,185,4],[186,3,186,4],[187,3,187,4],[188,3,188,4],[189,3,189,4],[190,3,190,4],[191,3,191,4],[192,3,192,4],[193,3,193,4],[194,0,194,6],[195,0,195,6],[196,0,196,3],[196,4,196,6],[197,0,197,6],[198,0,198,3],[198,4,198,6],[199,0,201,0],[199,1,201,1],[199,2,201,2],[199,3,201,4],[199,5,201,5],[199,6,201,6],[202,3,202,4],[203,3,203,4],[204,3,204,4],[205,3,205,4],[206,3,206,4],[207,3,207,4],[208,3,208,4],[209,3,209,4],[210,0,210,6],[211,0,211,6],[212,0,212,3],[212,4,212,6],[213,0,213,6],[214,0,214,3],[214,4,214,6],[215,0,217,0],[215,1,217,1],[215,2,217,2],[215,3,217,4],[215,5,217,5],[215,6,217,6],[218,3,218,4],[219,3,219,4],[220,3,220,4],[221,3,221,4],[222,3,222,4],[223,3,223,4],[224,3,224,4],[225,3,225,4],[226,3,226,4],[227,3,227,4],[228,3,228,4],[229,3,229,4],[230,3,230,4],[231,3,231,4]],"flags":["formulas_cached_only"]}
["分部分项工程和单价措施项目清单与计价表"]
["工程名称：门岗",{"$nulls":3},"标段：商水县公交车公司停车场配套设施门岗及厕所"]
["序号","项目编码","项目名称","项目特征描述",null,"计量单位","工程量"]
[]
[]
[null,"A.1","土石方工程"]
[1,"010101001001","平整场地","1.土壤类别:一、二类土\n2.弃土运距:1km内",null,"m2","28.91"]
[2,"010101002001","挖一般土方","1.土壤类别:一、二类土\n2.挖土深度:1.2米\n3.弃土运距:1km内",null,"m3","33.53"]
[3,"010103001001","回填方",null,null,"m3","23.41"]
[4,"010103002001","余方弃置","1.废弃料品种:一、二类土\n2.运距:1km以内",null,"m3","10.12"]
[null,null,"分部小计"]
[null,"A.4","砌筑工程"]
[1,"010401001001","砖基础","1.砖品种、规格、强度等级:MU15煤矸石实心砖\n2.基础类型:阶梯形\n3.砂浆强度等级:M10",null,"m3","3.5"]
[2,"010401003001","实心砖墙","1.砖品种、规格、强度等级:MU15煤矸石实心砖\n2.墙体类型:外墙 240mm\n3.砂浆强度等级、配合比:M7.5",null,"m3","13.18"]
[null,null,"分部小计"]
[null,"A.5","混凝土及钢筋混凝土工程"]
[1,"010501002001","带形基础","1.混凝土种类:商砼\n2.混凝土强度等级:C15\n3.部位:隔墙下基层",null,"m3","0.9"]
[2,"010502002001","构造柱","1.混凝土种类:商砼\n2.混凝土强度等级:C25",null,"m3","1"]
["本页小计"]
["注：为计取规费等的使用，可在表中增设其中：“定额人工费”。"]
[]
["分部分项工程和单价措施项目清单与计价表"]
["工程名称：门岗",{"$nulls":3},"标段：商水县公交车公司停车场配套设施门岗及厕所"]
["序号","项目编码","项目名称","项目特征描述",null,"计量单位","工程量"]
[]
[]
[3,"010503004001","圈梁","1.混凝土种类:商砼\n2.混凝土强度等级:C30\n3.部位:圈梁及雨棚梁",null,"m3","2.22"]
[4,"010503005001","过梁","1.混凝土种类:商砼\n2.混凝土强度等级:C25",null,"m3","0.12"]
[5,"010505003001","平板","1.混凝土种类:商砼\n2.混凝土强度等级:C30\n3.部位:现浇板",null,"m3","3.15"]
[6,"010505008001","雨篷","1.混凝土种类:商砼\n2.混凝土强度等级:C30\n3.部位:雨篷",null,"m3","0.17"]
[7,"010507001001","散水、坡道",null,null,"m2","20.47"]
[8,"010507004001","台阶","台阶做法\n12YJ9-1\n4/102",null,"m2","0.77"]
[9,"010507005001","扶手、压顶","1.断面尺寸:女儿墙压顶\n2.混凝土种类:商砼\n3.混凝土强度等级:C25",null,"m3","0.73"]
[10,"010515001001","现浇构件钢筋","1.钢筋种类、规格:圆钢筋 钢筋HPB300 直径 ≤10mm",null,"t","0.014"]
[11,"010515001002","现浇构件钢筋","1.钢筋种类、规格:带肋钢筋HRB400以内 直径 ≤10mm",null,"t","0.198"]
[12,"010515001003","现浇构件钢筋","1.钢筋种类、规格:带肋钢筋HRB400以内 直径 ≤18mm",null,"t","0.436"]
[13,"010515001004","现浇构件钢筋","带肋钢筋HRB400以内 直径 ≤25mm",null,"t","0.016"]
["本页小计"]
["注：为计取规费等的使用，可在表中增设其中：“定额人工费”。"]
[]
["分部分项工程和单价措施项目清单与计价表"]
["工程名称：门岗",{"$nulls":3},"标段：商水县公交车公司停车场配套设施门岗及厕所"]
["序号","项目编码","项目名称","项目特征描述",null,"计量单位","工程量"]
[]
[]
[14,"010515001005","现浇构件钢筋","1.钢筋种类、规格:箍筋 圆钢HPB300 直径 ≤10mm",null,"t","0.061"]
[15,"010515001006","现浇构件钢筋","1.钢筋种类、规格:箍筋 带肋钢筋HRB400以内 直径 ≤10",null,"t","0.054"]
[16,"010515001007","现浇构件钢筋","1.钢筋种类、规格:砌体内加固钢筋",null,"t","0.086"]
[null,null,"分部小计"]
[null,"A.8","门窗工程"]
[1,"010802004001","防盗门","1.门代号及洞口尺寸:M1121,M1125\n2.门框、扇材质:双层复合防盗门",null,"m2","5.06"]
[2,"010807001001","金属（塑钢、断桥）窗","1.窗代号及洞口尺寸:C1518,C2021\n2.框、扇材质:白色塑钢中空窗带纱扇\n3.玻璃品种、厚度:5+9A+5",null,"m2","11.1"]
[null,null,"分部小计"]
[null,"A.9","屋面及防水工程"]
[1,"010902001001","屋面卷材防水","不上人屋面-水泥砂浆保护层屋面(参12YJ1\n1·20厚1:2.5水泥砂浆保护层\n2·0.4厚聚乙烯膜一层\n3·4厚高聚物改性沥青卷材防水(SBS)一道\n4·30厚C20细石混凝土找平层\n5·100厚挤塑聚苯板保温层\n6·20厚1:2.5水泥砂浆找平层\n7·最薄处30厚泡沫混凝土找2%坡\n8·现浇钢筋混凝土楼板",null,"m2","23.35"]
["本页小计"]
["注：为计取规费等的使用，可在表中增设其中：“定额人工费”。"]
[]
["分部分项工程和单价措施项目清单与计价表"]
["工程名称：门岗",{"$nulls":3},"标段：商水县公交车公司停车场配套设施门岗及厕所"]
["序号","项目编码","项目名称","项目特征描述",null,"计量单位","工程量"]
[]
[]
[2,"010902002001","屋面涂膜防水","雨篷等屋面：\n1.保护层:20厚1:2水泥砂浆抹面压光,找坡1%\n2.防水层:1.5厚水泥基防水涂料上翻150\n3.结构层:现浇钢筋混凝土屋面板",null,"m2","1.7"]
[3,"010902004001","屋面排水管","1.排水管品种、规格:塑料(PVC)",null,"m","6.6"]
[null,null,"分部小计"]
[null,"A.11","楼地面装饰工程"]
[1,"011102003001","块料楼地面","陶瓷地砖地面地面，做法12YJ1地201",null,"m2","23.41"]
[null,null,"分部小计"]
[null,"A.12","墙、柱面装饰与隔断、幕墙工程"]
[1,"011201001001","内墙抹灰","1.墙体类型:内墙\n2.混合砂浆墙面\n3.做法详12YJ1内墙3C",null,"m2","67.22"]
[2,"011201001002","外墙抹灰","1.墙体类型:内墙\n2.混合砂浆墙面\n3.做法详12YJ1",null,"m2","79.78"]
[null,null,"分部小计"]
[null,"A.13","天棚工程"]
[1,"011301001001","天棚抹灰","混合砂浆顶棚，做法详12YJ1顶5涂304",null,"m2","22.89"]
[null,null,"分部小计"]
[null,"A.14","油漆、涂料、裱糊工程"]
[1,"011407001001","外墙墙面喷刷涂料","1.涂料品种、喷刷遍数:真石漆",null,"m2","79.78"]
[2,"011407001002","内墙墙面喷刷涂料","做法详12YJ1涂304",null,"m2","22.88"]
[3,"011407002001","天棚喷刷涂料",null,null,"m2","22.88"]
[4,"01B001","砼泵送费",null,null,"m3","96.62"]
[null,null,"分部小计"]
["本页小计"]
["注：为计取规费等的使用，可在表中增设其中：“定额人工费”。"]
[]
["分部分项工程和单价措施项目清单与计价表"]
["工程名称：门岗",{"$nulls":3},"标段：商水县公交车公司停车场配套设施门岗及厕所"]
["序号","项目编码","项目名称","项目特征描述",null,"计量单位","工程量"]
[]
[]
[null,null,"大西环办公楼门口硬化"]
[1,"060104008001","砖渣机械碾压","1.碾压厚度:25CM\n2.填料种类:砖渣",null,"m2","379.05"]
[2,"040203007001","水泥混凝土","1.混凝土强度等级:C30\n2.厚度:22CM",null,"m2","379.05"]
[null,null,"分部小计"]
[null,null,"电气"]
[1,"030404017001","配电箱","1.名称:照明配电箱\n2.规格:PZ30",null,"台","1"]
[2,"030412001001","普通灯具","1.名称:声光控型防水防尘灯\n2.规格:28W",null,"套","3"]
[3,"030411001001","配管","1.名称:PC16",null,"m","28.7"]
[4,"030411004001","配线","1.规格:BV-3*2.5",null,"m","86.1"]
[null,null,"分部小计"]
[null,null,"措施项目"]
[1,"011701001001","综合脚手架",null,null,"m2","28.94"]
[2,"011705001001","大型机械设备进出场及安拆",null,null,"台·次","1"]
[3,"011702003002","构造柱",null,null,"m2","20.94"]
[4,"011702008001","圈梁",null,null,"m2","31.47"]
[5,"011702016001","平板",null,null,"m2","28.89"]
[6,"011702023001","雨篷、悬挑板、阳台板",null,null,"m2","2.24"]
[7,"011702009001","过梁",null,null,"m2","1.66"]
["分部分项工程和单价措施项目清单与计价表"]
["工程名称：公共厕所",{"$nulls":3},"标段：商水县公交车公司停车场配套设施门岗及厕所"]
["序号","项目编码","项目名称","项目特征描述",null,"计量单位","工程量"]
[]
[]
[null,null,"土建"]
[null,"A.1","土石方工程"]
[1,"010101001001","平整场地","1.土壤类别:一、二类土\n2.弃土运距:自行考虑",null,"m2","59.00"]
[2,"010101003001","挖沟槽土方","1.土壤类别:一、二类土\n2.挖土深度:按设计要求结合施工现场场地情况\n3.弃土运距:自行考虑",null,"m3","33.76"]
[3,"010103001001","回填方","1.密实度要求:夯填\n2.填方材料品种:素土\n3.填方粒径要求:符合设计要求\n4.填方来源、运距:自行考虑",null,"m3","20.51"]
[null,"A.4","砌筑工程"]
[1,"010401001001","砖基础","1.砖品种、规格、强度等级:MU15煤矸石实心砖\n2.砂浆强度等级:M10水泥砂浆",null,"m3","4.8114"]
[2,"010401003001","实心砖墙","1.砖品种、规格、强度等级:烧结煤矸石普通砖\n2.砂浆强度等级、配合比:M7.5混合砂浆",null,"m3","22.5864"]
[3,"010401012001","女儿墙","1.砖品种、规格、强度等级:烧结煤矸石普通砖\n2.砂浆强度等级、配合比:M7.5混合砂浆",null,"m3","2.8512"]
[null,"A.5","混凝土及钢筋混凝土工程"]
[1,"010501001001","垫层","1.混凝土种类:商品\n2.混凝土强度等级:C15",null,"m3","2.60"]
["本页小计"]
["注：为计取规费等的使用，可在表中增设其中：“定额人工费”。"]
[]
["分部分项工程和单价措施项目清单与计价表"]
["工程名称：公共厕所",{"$nulls":3},"标段：商水县公交车公司停车场配套设施门岗及厕所"]
["序号","项目编码","项目名称","项目特征描述",null,"计量单位","工程量"]
[]
[]
[2,"010501002001","带形基础","1.混凝土种类:商品\n2.混凝土强度等级:C30",null,"m3","5.8428"]
[3,"010502002001","构造柱","1.混凝土种类:商品\n2.混凝土强度等级:C30",null,"m3","2.016"]
[4,"010503004001","圈梁","1.混凝土种类:商品\n2.混凝土强度等级:C30",null,"m3","3.4214"]
[5,"010505001001","有梁板","1.混凝土种类:商品\n2.混凝土强度等级:C30",null,"m3","4.5"]
[6,"010507001001","散水","1.散水详见05YJ9-1",null,"m2","26.73"]
[7,"010507001002","坡道","1.坡道详见12YJ1-地201",null,"m2","1.98"]
[8,"010507005001","扶手、压顶","1.混凝土种类:商品\n2.混凝土强度等级:C30",null,"m3","1.276"]
[9,"010515001002","现浇构件钢筋","1.钢筋种类、规格:现浇构件带肋钢筋 带肋钢筋HRB400以内 直径 ≤10mm",null,"t","0.5"]
[10,"010515001003","现浇构件钢筋","1.钢筋种类、规格:箍筋 带肋钢筋HRB400以内 直径 ≤10mm",null,"t","0.15"]
[11,"010515001005","现浇构件钢筋","1.钢筋种类、规格:砌体内加固钢筋",null,"t","0.11"]
[null,"A.8","门窗工程"]
[1,"010807001001","金属（塑钢、断桥）窗","1.窗代号及洞口尺寸:1208\n2.框、扇材质:塑钢窗",null,"m2","3.84"]
[null,"A.9","屋面及防水工程"]
[1,"010902001001","屋面卷材防水","不上人无保温平屋面做法详见12YJ1-屋108-2F1",null,"m2","41.5776"]
["本页小计"]
["注：为计取规费等的使用，可在表中增设其中：“定额人工费”。"]
[]
["分部分项工程和单价措施项目清单与计价表"]
["工程名称：公共厕所",{"$nulls":3},"标段：商水县公交车公司停车场配套设施门岗及厕所"]
["序号","项目编码","项目名称","项目特征描述",null,"计量单位","工程量"]
[]
[]
[2,"010902004001","屋面排水管","1.排水管品种、规格:屋面排水 塑料管排水 水落管φ≤110mm\n2.落水斗1个\n3.弯头落水口1个",null,"m","3.5"]
[null,"A.11","楼地面装饰工程"]
[1,"011102003001","块料楼地面","1.300*300陶瓷地砖防水地面做法详见12YJ1地201F-F1",null,"m2","41.92"]
[null,"A.12","墙、柱面装饰与隔断、幕墙工程"]
[1,"011201001001","墙面一般抹灰","1.墙体类型:外墙\n2.面层厚度、砂浆配合比:干混抹灰砂浆",null,"m2","91.46"]
[2,"011201001002","墙面一般抹灰","1.墙体类型:内墙\n2.面层厚度、砂浆配合比:干混抹灰砂浆",null,"m2","52.448"]
[3,"011204003001","块料墙面","1.300*450釉面砖墙裙，高1.8m,做法详见12YJ1-裙3AF-F1",null,"m2","76.032"]
[4,"011210005001","成品隔断","1.隔断材料品种、规格、颜色:成品隔断",null,"m2","9.54"]
[null,"A.14","油漆、涂料、裱糊工程"]
[1,"011406001001","抹灰面油漆","1.油漆品种、刷漆遍数:真石漆 墙面",null,"m2","91.46"]
[2,"011407001001","墙面喷刷涂料","1.白色仿瓷涂料两遍做法详见12YJ1内墙2",null,"m2","52.448"]
[3,"011407002001","天棚喷刷涂料","1.涂料顶棚，做法12YJ1顶2涂304",null,"m2","42.68"]
[null,"A.15","其他装饰工程"]
[1,"011505001001","洗漱台","1.材料品种、规格、颜色:大理石洗漱台 >1m2\n2.台面开孔4个",null,"m2","1.86"]
[null,"A.17","措施项目"]
["本页小计"]
["注：为计取规费等的使用，可在表中增设其中：“定额人工费”。"]
[]
["分部分项工程和单价措施项目清单与计价表"]
["工程名称：公共厕所",{"$nulls":3},"标段：商水县公交车公司停车场配套设施门岗及厕所"]
["序号","项目编码","项目名称","项目特征描述",null,"计量单位","工程量"]
[]
[]
[1,"011702001001","基础","1.基础类型:垫层模板\n2.具体规格做法详见相关规范规定",null,"m2","6.492"]
[2,"011702001002","带形基础","1.带形基础模板\n2.具体规格做法详见相关规范规定",null,"m2","19.476"]
[3,"011702003001","构造柱","1.构造柱模板\n2.具体规格做法详见相关规范规定",null,"m2","26.88"]
[4,"011702008001","圈梁","1.圈梁模板\n2.具体规格做法详见相关规范规定",null,"m2","14.256"]
[5,"011702014001","有梁板","1.有梁板模板\n2.具体规格做法详见相关规范规定",null,"m2","45"]
[6,"011702028001","压顶模板","1.压顶模板\n2.具体规格做法详见相关规范规定",null,"m2","1.189"]
[null,null,"分部小计"]
[null,null,"电气"]
[null,"C.4","电气设备安装工程"]
[1,"030404017001","配电箱","1.名称:照明配电箱\n2.规格:PZ30",null,"台","1"]
[2,"030411001001","配管","1.名称:PC16",null,"m","28.7"]
[3,"030411004001","配线","1.规格:BV-3*2.5",null,"m","86.1"]
[4,"030412001001","普通灯具","1.名称:声光控型防水防尘灯\n2.规格:28W",null,"套","3"]
[null,null,"分部小计"]
[null,null,"给排水"]
[null,"C.10","给排水、采暖、燃气工程"]
[1,"031001006001","塑料管","1.介质:给水\n2.材质、规格:De50\n3.连接形式:热熔连接\n4.压力试验及吹、洗设计要求:消毒冲洗",null,"m","3.3"]
["本页小计"]
["注：为计取规费等的使用，可在表中增设其中：“定额人工费”。"]
[]
["分部分项工程和单价措施项目清单与计价表"]
["工程名称：公共厕所",{"$nulls":3},"标段：商水县公交车公司停车场配套设施门岗及厕所"]
["序号","项目编码","项目名称","项目特征描述",null,"计量单位","工程量"]
[]
[]
[2,"031001006002","塑料管","1.介质:给水\n2.材质、规格:De40\n3.连接形式:热熔连接\n4.压力试验及吹、洗设计要求:消毒冲洗",null,"m","20.3"]
[3,"031001006003","塑料管","1.介质:给水\n2.材质、规格:De25\n3.连接形式:热熔连接\n4.压力试验及吹、洗设计要求:消毒冲洗",null,"m","9.9"]
[4,"031001006004","塑料管","1.介质:给水\n2.材质、规格:De20\n3.连接形式:热熔连接\n4.压力试验及吹、洗设计要求:消毒冲洗",null,"m","2.3"]
[5,"031001006005","塑料管","1.介质:给水\n2.材质、规格:De15\n3.连接形式:热熔连接\n4.压力试验及吹、洗设计要求:消毒冲洗",null,"m","5.4"]
[6,"031001006006","塑料管","1.介质:污水\n2.材质、规格:DN50\n3.连接形式:粘接",null,"m","5"]
[7,"031001006007","塑料管","1.介质:污水\n2.材质、规格:De75\n3.连接形式:粘接",null,"m","4"]
[8,"031001006008","塑料管","1.介质:污水\n2.材质、规格:DN100\n3.连接形式:粘接",null,"m","20.8"]
[9,"031003001001","螺纹阀门","1.类型:闸阀\n2.规格、压力等级:DN50",null,"个","1"]
["本页小计"]
["注：为计取规费等的使用，可在表中增设其中：“定额人工费”。"]
[]
["分部分项工程和单价措施项目清单与计价表"]
["工程名称：公共厕所",{"$nulls":3},"标段：商水县公交车公司停车场配套设施门岗及厕所"]
["序号","项目编码","项目名称","项目特征描述",null,"计量单位","工程量"]
[]
[]
[10,"031003001002","螺纹阀门","1.类型:止回阀\n2.规格、压力等级:DN50",null,"个","1"]
[11,"031003013001","水表","1.型号、规格:DN50",null,"个","1"]
[12,"031004003001","洗脸盆","1.材质:洗脸盆",null,"组","4"]
[13,"031004006001","大便器","1.材质:蹲式大便器",null,"组","9"]
[14,"031004006002","大便器","1.材质:坐式大便器",null,"组","1"]
[15,"031004007001","小便器","1.材质:挂式小便器",null,"组","6"]
[16,"031004008001","其他成品卫生器具","1.材质:拖布池",null,"组","1"]
[17,"031004014001","给、排水附(配)件","1.材质:地漏",null,"个","3"]
[null,"D.5","管网工程"]
[1,"040504001001","砌筑井",null,null,"座","1"]
[2,"040504008001","化粪池","35m3砖砌化粪池4*3.6*3m",null,"座","1"]
[null,null,"分部小计"]
[null,null,"措施项目"]
[1,"011701001001","综合脚手架",null,null,"m2","48.54"]

{"sheet":"Sheet2","index":1,"n_rows":0,"n_cols":0,"rows_kept":0,"flags":["formulas_cached_only"]}

{"sheet":"Sheet3","index":2,"n_rows":0,"n_cols":0,"rows_kept":0,"flags":["formulas_cached_only"]}